1. Board Manager -> ESP8266 by community 2.7.4로 다운그레이드
2. https://www.grc.com/fingerprints.htm

“6E:F3:55:47:6D:F1:0E:5B:2B:04:F2:F8:C0:8B:E8:05:65:0F:1A:C1”

* <https://medium.com/@bimxra/how-to-fix-nodemcu-arduino-firebase-library-not-working-issue-5c8ff5a4a1ff>

3. PYSERIAL OR ESPTOOL DIRECTORIES NOT FOUND

* <https://www.tweaking4all.com/forum/arduino/macos-aruino-ide-how-to-fix-pyserial-or-esptool-directories-not-found-next-to-this-upload-py-tool-error-esp8266/>
* <https://www.esp8266.com/viewtopic.php?f=32&t=21692&start=4>